{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Main","Help","Table of Values"],"not_rendered":{"charts":0,"images":9,"macros":1,"external_links":0,"defined_names":5,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Main","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[]}
["CEEN 270-Open Steady Channel Flow Calculator"]
["By Matthew Bayles and Mark Bester"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"n=",1.2999999999999999E-2,"Slope=",4.523153867192653E-5]
[null,"Q=",1,"ft^3/s"]
[null,"b=",1,"ft"]
[null,"z=",1,"ft"]
[null,"y=",1,"ft"]

{"sheet":"Help","index":1,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["CEEN 270-Open Steady Channel Flow Calculator"]
["By Matthew Bayles and Mark Bester"]

{"sheet":"Table of Values","index":2,"n_rows":13,"n_cols":4,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Rectangle",null,"Glass, Copper, or Plastic",0.01]
["Triangle",null,"Smmoth, Unpainted Steel, Planned Wood",1.2E-2]
["Trapezoid",null,"Painted Steel or Coated Cast Iron",1.2999999999999999E-2]
["Circular",null,"Smooth Asphalt or Clay",1.4E-2]
[null,null,"Uncoated Cast Iron or Iron Pipe",1.4999999999999999E-2]
[null,null,"Brick in Cement Mortar",1.7000000000000001E-2]
[null,null,"Formed Concrete",1.7999999999999999E-2]
[null,null,"Smooth Earth",2.1999999999999999E-2]
[null,null,"Clean Excavated Earth",2.4E-2]
[null,null,"Corrugated Metal Storm Drain",0.03]
[null,null,"Natural Channel with Stones and Weeds",0.05]
[null,null,"Natural Channel With Tall Grasses and Reeds",0.06]
[null,null,"Natural Channel with Heavy Brush",0.1]